{"text_format":"3","workbook":"xlsx","n_sheets":1,"sheets":["Sheet1"],"read":"whole","date_system":"1900"}

{"sheet":"Sheet1","index":0,"n_rows":36,"n_cols":5,"rows_kept":36,"merged":[[0,0,0,4]]}
["基础教学与实训中心科研实验耗材采购清单"]
["序号","名称","型号/描述","数量","备注"]
[1,"核心控制器模块","ESP32（240MHz 双核）、16MFLASH、4M PSRAM",15]
[2,"温度/湿度/气压传感器","DHT12 温湿度单元，BMP280 气压计，I2C 接口",10]
[3,"红外线发射接收单元","红外线发射/接收电器遥控，红外距离传感，GPIO 接口",15]
[4,"RGB 单元","3 颗 RGB 彩灯，GPIO 接口",10]
[5,"摄像头单元","200W 像素、含 ESP32/PSRAM、有 GROVE 引出、能内置 MPU9250、USB/GROVE 供电",5]
[6,"3轴步进电机驱动模块","3 轴步进电机驱动、带 GRBL 内核，可二次开发、含电源/散热层、I2C 接口",5]
[7,"GSM 模块","SIM800 实现 GSM/GPRS 功能、UART 接口",10]
[8,"GPS/北斗 定位模块","M8N GPS、带内置/外置GPS 天线、UART 接口",5]
[9,"便携套件","含键盘/计数器/面板、可挂墙充电底座",5]
[10,"LoRa 通讯模块","433MHz LoRa 通信",10]
[11,"通信扩展模块","CAN/485/TTL/I2C 通讯扩展层",10]
[12,"LAN 通讯模块","W5500 LAN 通讯方案、带 24V->5V 电源转换、DINRail 安装部件、含 3.96 扩展接口",10]
[13,"stivc控制器","esp32芯片、lcd屏、3个按钮、内置9轴陀螺仪、led状态灯",10]
[14,"PLC 控制底座","带 24V->5V 电源转换、485 转换小板、DINRail 安装部件、2.54 扩展、含3.96 扩展接口",10]
[15,"3.96 扩展单元","Grove-3.96 直通、GPIO接口",10]
[16,"扩展空板","2.54 间距扩展层模块",15]
[17,"PROTO 扩展单元","2.54 间距、GPIO 接口",10]
[18,"可调电阻单元","可调电阻、I2C 控制",10]
[19,"分接单元","HUB 扩展、I2C 控制",10]
[20,"继电器单元","3A 继电器、交流 220V3A、直流 30V3A、含三极管驱动、3.96 端子、GPIO 接口",15]
[21,"按钮单元","含轻触按钮、GPIO 接口",10]
[22,"双按键单元","含 2 个轻触按钮、GPIO 接口",10]
[23,"亮度单元","光敏电阻、含模拟及开关量通道、电位器调节阀值、GPIO 接口",10]
[24,"PA—HUB模块","I2C总线拓展接口至少6路（可定义分配同种传感器不同地址）",10]
[25,"PB-HUB模块","普通IO拓展接口，至少6路（可定义分配同种传感器不同地址）",10]
[26,"传感器套装","StickV、FACE-RFID、FACE-Finger、 RGBLED、Servo Module 舵机",10]
[27,"伺服电机","转角反馈精度0.5度，160—170rpm，20N/cm\n运行扭矩，40N/cm静态转矩，直流电压10V",4]
[28,"摄像头单元","集成ESP32（4M Flash + 520K RAM + 4M PSRAM）\n芯片和200万像素的摄像头（OV2640）.支持\nWiFi-图像传输和USB端口调试.CP2104 USB TTL\nOV2640 传感器\n输出格式（8位）:\n8- / 10位Raw RGB数据\n根据特定格式的最大图像传输速率\nUXGA/SXGA: 15fps\nSVGA: 30fps\nCIF: 60fps\n扫描模式: 渐进式\n相机规格\nCCD 尺寸 : 1/4 inch\n视野 : 65 °\n最大像素: 2M\n传感器最佳分辨率: 1600 * 1200\n尺寸: 40 × 49 × 13mm",5]
[29,"LOT套件","ESP32开发板  Arduino物联网开发工具STEM  ",8]
[30,"FIRE模块","双模蓝牙、esp32开发板套件高性能PSRAM、2.4G天线M5G0底座",6]
[31,"ATOM Matrix模块","MPU6886 Arduino、内置3轴陀螺仪和3轴加速计、5*5RGB LED点阵屏",10]
[32,"ATOM Lite模块","嵌入式智能硬件开发板3D天线带Wi-Fi 、内置红外发射功能、可扩展的引脚与接口、按键G39",10]
[33,"鱼眼广角摄像头","PSRAM OV2640开发板带WIFi蓝牙、4M Flash+520k RAM+4M PSRAM",8]
[34,"高精度激光测距传感器","内部集成ST激光测距芯片VL53L0X",5]